1. Types
2. appliance
3. techpreview
4. networking
5. routes

## appliance techpreview networking routes: route

`route` structure Structure that describes how routing is performed for a particular destination and prefix. A destination/prefix of 0.0.0.0/0 ( for IPv4) or ::/0 (for IPv6) refers to the default gateway.

### Representations:

- JSON
- XML

{
"destination": "string",
"gateway": "string",
"interface_name": "string",
"prefix": 1
}
<?xml version="1.0" ?>
<ns0:Route xmlns:ns0="http://vmware.com/appliance/techpreview/networking/routes" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">
<gateway>string</gateway>
<prefix>1</prefix>
<interface_name>string</interface_name>
<destination>string</destination>
</ns0:Route>

#### Attributes:

Name | Type | Description
--- | --- | ---
Required
destination | string | Destination address that defines this route.
prefix | long | Destination CIDR prefix that defines this route. See http://www.oav.net/mirrors/cidr.html for netmask-to-prefix conversion.
gateway | string | Gateway address.
interface_name | string | Output device interface, for example, "nic0".