1. Operations
2. appliance
3. access
4. ssh

## appliance access ssh: set

Set enabled state of the SSH-based controlled CLI.

### Request:

#### HTTP request

PUT https://{server}/rest/appliance/access/ssh

#### Request Body Structure:

- JSON
- XML

{
"enabled": true
}
<?xml version="1.0" ?>
<ns0:Set-Input xmlns:ns0="http://vmware.com/appliance/access/ssh" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">
<enabled>true</enabled>
</ns0:Set-Input>

#### Request Body Parameters:

Name | Type | Description
--- | --- | ---
bold = required
enabled | boolean | SSH-based controlled CLI is enabled.

### Response:

#### HTTP Status Code: 200

None

#### Errors:

HTTP Status Code | Type | Description
--- | --- | ---
500 | error | Generic error