1. Operations
2. appliance
3. techpreview
4. ntp
5. server

## appliance techpreview ntp server: add

Add NTP servers. This command adds NTP servers to the configuration. If the time synchronization is NTP-based, then NTP daemon is restarted to reload the new NTP servers. Otherwise, this command just adds servers to the NTP configuration.

### Request:

#### HTTP request

POST https://{server}/rest/appliance/techpreview/ntp/server

#### Request Body Structure:

- JSON
- XML

{
"servers": [
"string",
"string"
]
}
<?xml version="1.0" ?>
<ns0:Add-Input xmlns:ns0="http://vmware.com/appliance/techpreview/ntp/server" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">
<servers-array>
<array-item>string</array-item>
<array-item>string</array-item>
</servers-array>
</ns0:Add-Input>

#### Request Body Parameters:

Name | Type | Description
--- | --- | ---
bold = required
servers | string[] | List of host names or IP addresses of NTP servers.

### Response:

#### HTTP Status Code: 200

None

#### Errors:

HTTP Status Code | Type | Description
--- | --- | ---
500 | error | Generic error