D-Link Print Server - Advanced Print

Product Page: DPR-1260 | Firmware Version: 1.24

| Status | Scan | Advanced | Setup | Help

- Printing
- Wireless
- System

# Advanced Printing

The following settings determine which printing protocols are enabled on the print server. The print server will listen for print jobs on the TCP ports associated with the enabled protocols.

## Printing Protocol

Raw TCP Port | Enable Disable
LPR/LPD | Enable Disable

Helpful Hints..
Printing Protocol:
Both protocols are enabled by default.
Raw TCP Port is the most common print method. This protocol uses TCP ports 9100-9103. Enable the protocol to communicate with an attached printer using the print server name and the unique TCP port number assigned to the printer.
LPR/LPD is more commonly used in Mac or Unix environments. This protocol uses TCP port 515. Enable the protocol to communicate with an attached printer using the print server name and the unique queue name assigned to the printer.

Copyright © 2006 D-Link Systems, Inc.