DWL-2700AP

Tools
Administrator Settings

Administrator settings allow you to customize User Name and Passwords as an Administrator of DWL-2700AP. The default value of the Username is "admin" with no password entered.

Password
Enter a password in the Access Point Password field. Type the password again in the next field to confirm it. The Password is case-sensitive ("A" is a different character than "a",) and must be between 0 and 12 characters in length.

System Settings
You may reset the DWL-2700AP back to factory settings by clicking on Restore Default settings. Restore Default Settings Choose Yes and click Apply to restore all Access Point settings to the factory default settings.
Firmware upgrade

This process allows users to download the latest files compatible to this particular device. Firmware upgrade may contain information for this device to fix any problems acquired in the past. Please visit http://support.dlink.com for the latest firmware for this device.

Update firmware From Local Hard Drive
After you have downloaded a firmware upgrade to your local drive, click Browse. Select the firmware and click Apply to complete the upgrade.

Configuration File
Update Configuration File Download Configuration File
Miscellaneous

Telnet Setting
User can disable or enable Telnet function for DWL-2700AP and specify telnet duration allowed. The default value of Telnet function is "enable" with timeout default "3 Minutes".

SNMP
SNMP default is disable , once user would like use SNMP Protocol based Manage tool , Please enable this function.