dlink-a389e6

Maintenance
Admin Password The administrator's password is changed here. Enter in the current password first and then the new password. Type in the new password again and click 'Save Settings' to put the change into effect.

System
Restart Click 'Restart' to reboot the DNS-343.
Defaults
Click 'Restore' to reset the DNS-343 to factory default settings. Use the restore feature only if necessary as this will erase all previously saved settings on the unit. This process will not harm or change any data on the internal drives.
Shutdown
Power off the unit.
Configuration Settings
Save configuration settings by pressing the 'Save' button and choosing a location for the configuration file to save to.
Load configuration settings by pressing the 'Browse' button to find the configuration file, then pressing the 'Load' button to load the file.
Idle Time
Enter a value for the System Inactivity Timer. If the administrator is idle for longer than the specified time, he will be logged out of the configuration area.
Enter a value for the Download Schedule Inactivity Timer. If a user is idle for longer than the specified time, he will be logged out of the Schedule Download area. Click 'Apply' when finished.

Firmware You can upgrade the firmware of the device from this page. The firmware you want to use must be saved on the local hard drive of the computer you are working from. Click on 'Browse' to search the local hard drive for the firmware to be used for the update. Click 'Apply' to begin the upgrade. Please check the D-Link support site for firmware updates at D-Link Support Page.

E-Mail Alerts
Login Method
Select 'Account' if your SMTP server requires authentication. Select 'Anonymous' if it does not.
User Name
If 'Account' is selected, enter the user name of your e-mail account.
Password
If 'Account' is selected, enter the password for your e-mail account.
SMTP Server
Enter the SMTP Server address. This will be your outgoing mail server address. If you're not sure what this is, contact the company that provides e-mail services for you.
Sender E-Mail
Enter the Sender's e-mail address. This is the address that the e-mail alerts will appear to be coming from.
Receiver E-Mail
Enter the Receiver's e-mail address. This is the address you want the e-mail alerts sent to.
Alert Types
Select the information you want e-mailed to the above address. The space status can be sent in intervals, while the other items will only be sent when necessary.
Click 'Save Settings' when finished.

Power Management
HDD Hibernation
Enable or Disable power management.
Turn Off Hard Drives
Select the amount of time before the hard drives will shut down. Remember that the device will stay powered on. Only the hard drives will lose power. They will re-gain power immediately after attempting to access them.
Click 'Save Settings' when finished.

Power Management
This section allows you to enable or disable the Hard Drive Hibernation and Power Recovery function.
HDD Hibernation
Select the amount of time before the hard drives will shut down. Remember that the device will stay powered on. Only the hard drives will lose power. They will re-gain power immediately after attempting to access them.
Power Recovery
If enabled, in the event of a power failure the DNS-343 will turn on and resume operation once power has been restored.
Click 'Save Settings' when finished.

Dynamic DNS
Enable this option only if you have purchased your own domain name and registered with a dynamic DNS service provider. The following parameters are displayed when the option is enabled.

Server Address
Select a dynamic DNS service provider from the pull-down list.
Host Name
Enter your host name, fully qualified; for example: myhost.mydomain.net.
Username or Key
Enter the username or key provided by your service provider. If the Dynamic DNS provider supplies only a key, enter that key in all three fields.
Password or Key
Enter the password or key provided by your service provider. If the Dynamic DNS provider supplies only a key, enter that key in all three fields.
Verify Password or Key
Re-type the password or key provided by your service provider. If the Dynamic DNS provider supplies only a key, enter that key in all three fields.
Status
Displays the current status of connection to DDNS server.

OLED Display Sleep When the OLED is idle, it will go into sleep mode after a pre-configured time ranging from 10 to 30 seconds and up to 1, 5, 10 and 15 minutes.

Disk Diagnostic
S.M.A.R.T Test
S.M.A.R.T stands for "Self-Monitoring, Analysis, and Reporting Technology". This is a system on a hard drive used to monitor and report on the health of the drive. If the HD is grayed out, then it does not support S.M.A.R.T.
In this section, you will be able to perform 2 tasks:
1. Run a Quick Test
2. Run an Extended Test
Quick Test - Runs a quick S.M.A.R.T test. The test usually takes less than 10 minutes. This test will check the electrical, mechanical, and read performance of the hard drive. The results are displayed as Passed/Failed on the web UI and can also be sent as an email alert.
Extended Test - Runs an extended S.M.A.R.T test. This test requires a lot more time to complete. However, it is a more thorough and complete test when compared to the Quick Test.
To run the S.M.A.R.T test, select the hard drive you wish to perform the S.M.A.R.T test on. Then select whether to run a Quick or Extended S.M.A.R.T test. Then press "Start" to run the test.
Send Result By Email
Enable this function in order to have the results of the S.M.A.R.T test sent to you by email.
Create Schedule
Click on this button in order to create a scheduled S.M.A.R.T test. You will be able to schedule a test on a daily, weekly, and monthly basis.
Scan Disk
Scan Disk will scan your system's file system for errors and/or corruption. After completion, any errors on your file system will be displayed accordingly.