D-LINK SYSTEMS, INC | WIRELESS ROUTER | HOME

Product Page: DIR-330 | Firmware Version: 1.12

| Setup | Advanced | Maintenance | Status | Help

- Port Forwarding
- Application Rules
- Network Filter
- Website Filter
- Firewall Settings
- advanced Wireless
- advanced Network
- Routing
- Certificates
- User Group

# Advanced Network Settings :

If you are not familiar with these Advanced Network settings, please read the help section before attempting to enable or disable them.

## UPnP :

Universal Plug and Play (UPnP) supports peer-to-peer Plug and Play functionality for network devices.

Enable UPnP : |

## WAN PING :

If you enable this feature, the WAN port of your router will respond to ping requests from the Internet that are sent to the WAN IP Address.

Enable WAN Ping Respond : |

## WAN port speed

WAN Port Speed : |

Helpful Hints.. For added security, it is recommended that you disable the WAN Ping Respond option. Ping is often used by malicious Internet users to locate active networks or PCs. If you are having trouble receiving multicast streams from the Internet, make sure the Multicast Stream option is enabled.

Copyright © 2004-2005 D-Link Systems, Inc.