D-LINK SYSTEMS, INC. | WIRELESS ROUTER : Status / Logs

Firmware Version: 1.32NA
Hardware Version: A4
Product Page: DIR-655

| Setup | Advanced | Tools | Status | Support

## Reboot needed

Your changes have been saved. The router must be rebooted for the changes to take effect. You can reboot now, or you can continue to make other changes and reboot later.

## Configuration Warnings

## Logs

Use this option to view the router logs. You can define what types of events you want to view and the event levels to view. This router also has internal syslog server support so you can send the log files to a computer on your network that is running a syslog utility.

Note: Only Administrator has access to these functionalities.

### Log Options

What to View : | Firewall & Security | System | Router Status
View Levels : | Critical | Warning | Informational

### Log Details

10 Log Entries:
Priority | Time | Message
--- | --- | ---
[INFO] | Sat Jan 31 10:43:23 2004 | Wireless link is up
[INFO] | Sat Jan 31 10:43:21 2004 | Allowed configuration authentication by IP address 192.168.0.11
[INFO] | Sat Jan 31 10:43:20 2004 | Starting DHCP server
[INFO] | Sat Jan 31 10:43:13 2004 | LAN interface is up
[INFO] | Sat Jan 31 10:43:13 2004 | LAN Ethernet Carrier Detected
[INFO] | Sat Jan 31 10:43:12 2004 | Device initialized
[WARN] | Sat Jan 31 10:43:11 2004 | Wireless schedule init
[INFO] | Sat Jan 31 10:43:11 2004 | guest: Unlock AP setup
[INFO] | Sat Jan 31 10:43:11 2004 | primary: Unlock AP setup
[INFO] | Sat Jan 31 10:43:11 2004 | No Internet access policy is in effect. Unrestricted Internet access allowed to everyone

Helpful Hints...

Check the log frequently to detect unauthorized network usage.

You can also have the log mailed to you periodically. Refer to Tools → EMail.

More...

Copyright © 2004-2008 D-Link Systems, Inc.