D-LINK SYSTEMS, INC. | WIRELESS ROUTER : Setup / Wireless Network Setup Wizard

Firmware Version: 1.13NA
Hardware Version: A1
Product Page: DIR-825

## Reboot needed

Your changes have been saved. The router must be rebooted for the changes to take effect. You can reboot now, or you can continue to make other changes and reboot later.

### Network Type

Private Select this option if you want to add a private network

The wireless network has been configured previously. Proceeding with this option will override these settings.

Guest Select this option if you want to add a guest network

### Configuration Method

Auto Select this option if your wireless device supports Wi-Fi Protected Setup.

Manual Select this option if you want to set up your network manually.

### Welcome to the Wireless Security Setup Wizard

This wizard will guide you through a step-by-step process to set up your wireless network and make it secure.

###

###

Your wireless network needs a name so it can be easily recognized by wireless clients. For security purposes, it is highly recommended to change the pre-configured network name.

Wireless Network Name (SSID) :

###

In order to protect your network from hackers and unauthorized users, it is highly recommended you choose one of the following wireless network security settings.

There are several levels of wireless security. The level you choose depends on the security features your wireless adapters support.

BEST Select this option if your wireless adapters SUPPORT WPA2

BETTER Select this option if your wireless adapters SUPPORT WPA

GOOD Select this option if your wireless adapters DO NOT SUPPORT WPA

NONE Select this option if you do not want to activate any security features

For information on which security features your wireless adapters support, please refer to the adapters' documentation.

###

You have selected your security level - you will need to set a wireless security password.

Wireless Security Password : (13 characters or 26 hex digits) (8 to 63 characters)

Note: You will need to enter the same password as keyed in this step into your wireless clients in order to enable proper wireless communication.

###

Your wireless network needs a name so it can be easily recognized by wireless clients. For security purposes, it is highly recommended to change the pre-configured network name.

Wireless Network Name (SSID) :

###

In order to protect your network from hackers and unauthorized users, it is highly recommended you choose one of the following wireless network security settings.

There are several levels of wireless security. The level you choose depends on the security features your wireless adapters support.

BEST Select this option if your wireless adapters SUPPORT WPA2

BETTER Select this option if your wireless adapters SUPPORT WPA

GOOD Select this option if your wireless adapters DO NOT SUPPORT WPA

NONE Select this option if you do not want to activate any security features

For information on which security features your wireless adapters support, please refer to the adapters' documentation.

###

You have selected your security level - you will need to set a wireless security password.

Wireless Security Password : (13 characters or 26 hex digits) (8 to 63 characters)

Note: You will need to enter the same password as keyed in this step into your wireless clients in order to enable proper wireless communication.

### Step 1: Welcome TO THE D-LINK WIRELESS SECURITY SETUP WIZARD

Give your network a name, using up to 32 characters.

| Network Name (SSID) 2.4GHz Band :
| Manually set 5GHz band Network Name (SSID)
| Network Name (SSID) 5GHz Band :

| Automatically assign a network key(Recommended)
| To prevent outsiders from accessing your network, the router will automatically assign a security to your network.
| Manually assign a network key
| Use this options if you prefer to create our own key.
| Use WPA encryption instead of WEP(WPA is stronger than WEP and all D-Link wireless client adapters support WPA)

Note: All D-Link wireless adapters currently support WPA.

### Step 2: Set your Wireless Security Password

You have selected your security level - you will need to set a wireless security password.

The WEP ( Wired Equivalent Privacy) key must meet one of following guildelines:

- Exactly 5 or 13 characters

- Exactly 10 or 26 characters using 0-9 and A-F

A longer WEP key is more secure than a short one

The WPA (Wi-Fi Protected Access) key must meet one of following guildelines:

- Between 8 and 63 characters (A longer WPA key is more secure than a short one)

- Exactly 64 characters using 0-9 and A-F

Use the same Wireless Security Password on both 2.4GHz and 5GHz band

2.4GHz Band Wireless Security Password :

5GHz Band Wireless Security Password :

Note: You will need to enter the same password as keys in this step into your wireless clients in order to enable proper wireless communication.

### Setup Complete!

Below is a detailed summary of your wireless security settings. Please print this page out, or write the information on a piece of paper, so you can configure the correct settings on your wireless client adapters.

Wireless Band : 2.4GHz Band

Wireless Network Name (SSID) : dir825

Wep Key Length : 128 bits

Default WEP Key to Use : 1

Authentication : Both

Wep Key :

Security Mode 1 : Auto (WPA or WPA2) - Personal

Cipher Type : TKIP and AES

Pre-Shared Key : 1234657488

Encryption : WPA2-PSK/AES (also known as WPA2 Personal)

Pre-Shared Key :

Security Mode 2 :

Cipher Type :

Pre-Shared Key :

Wireless Band : 5GHz Band

Wireless Network Name (SSID) : dlink_media

Wep Key Length : 128 bits

Default WEP Key to Use : 1

Authentication : Both

Wep Key :

Security Mode 1 : Auto (WPA or WPA2) - Personal

Cipher Type : TKIP and AES

Pre-Shared Key : 123456789

Encryption : WPA2-PSK/AES (also known as WPA2 Personal)

Pre-Shared Key :

Security Mode 2 :

Cipher Type :

Pre-Shared Key :

Copyright © 2004-2008 D-Link Systems, Inc.