D-LINK SYSTEMS, INC | WIRELESS ROUTER | HOME

Product Page: DIR-615 | Hardware Version: C1 | Firmware Version: 3.10NA |

| SETUP | ADVANCED | TOOLS | STATUS | SUPPORT

- Virtual Server
- Port Forwarding
- Application Rules
- QOS Engine
- Network Filter
- Access control
- Website Filter
- Inbound Filter
- Firewall Settings
- Routing
- Advanced Wireless
- Advanced Network
- IPv6

# QoS Engine

Use this section to configure D-Link's QoS Engine. The QoS Engine improves your online gaming experience by ensuring that your game traffic is prioritized over other network traffic, such as FTP or Web.

## WAN Traffic Shaping

Enable Traffic Shaping: |
Automatic Uplink Speed : |
Measured Uplink Speed : | Not Estimated
Manual Uplink Speed : | kbps <<

## QoS Engine Setup

Enable QoS Engine : |
Automatic Classification : |
Dynamic Fragmentation : |

Helpful Hints…

If the Measured Uplink Speed is known to be incorrect (that is, it produces suboptimal performance), disable Automatic Uplink Speed and enter the Manual Uplink Speed. Some experimentation and performance measurement may be required to converge on the optimal value.

More…

Copyright © 2004-2008 D-Link Systems, Inc.