dlink-6CE05B

Product Page: DNS-726-4 |  | Firmware Version: 1.00

| Live Video | Playback | Setup | Maintenance | Status | Help

- Wizard
- Network Setup
- Camera Search
- Camera Setup
- Audio and Video
- Live & Playback Setup
- Recording Schedule
- Event Setup
- E-Mail Setup
- Dynamic DNS
- Time and Date Setup
- Logout

# RECORDING SCHEDULE

You can set up individual cameras to record at specific times, day or night, one time or each day of the week.

## RECORDING MODE

No Record
Record by Schedule
Always Record Camera 1 Camera 2 Camera 3 Camera 4

## VIDEO DATA

Automatic Overwrite | Enable
Store Videos | Store Videos by Schedule Days

## RECORDING SCHEDULE

Camera List | Schedule

Day Week

01 02 03 04 05 06 07 08 09 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24
Cam1
Cam2
Cam3
Cam4
01 02 03 04 05 06 07 08 09 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24
Sun
Mon
Tue
Wed
Thur
Fri
Sat

Helpful Hints..

The following list briefly describes the Recording Schedule menu items:
Automatic Overwrite: Select this option to automatically empty disk space when the disk space is full. This will overwrite the earliest recorded video with the latest video one day at a time.
Store Videos by Schedule: Set duration to store recorded video clips. After this, the clips will be purged and cannot be recovered. Insert: Insert new schedules.
Delete: Delete the selected schedule.
Configure: Modify the schedule and recording mode setting.
Notes
- The Always Record option will start recording immediately.
- When configuring the Motion Detection event, ensure to setup the motion detection function in your camera first.
- When changing the motion detection settings of your camera, ensure to disconnect the NVR and then re-connect to update the settings in your NVR.
- When setting up an event, a video motion or digital input can be used to trigger the other cameras. This means that when motion is detected by a camera, it can send out warning signals to the other connected cameras.
- An alternative option is to drag the time bar to change the recording time period. The red bar represents the ��Always Record�� feature and the blue bar represents the ��Event Recording�� feature.

Copyright © 2008 D-Link Corporation/D-Link System, Inc.