D-LINK SYSTEMS, INC | WIRELESS ROUTER | HOME

Product Page : DIR-685

Hardware Version : A1

Firmware Version : 1.00NA

| Setup | Advanced | Storage | Tools | Status | Support

- Port Forwarding
- Application Rules
- QoS Engine
- Network Filter
- Website Filter
- Firewall Settings
- Routing
- Advanced Wireless
- Advanced Network
- Guest Zone
- Wake on LAN

# MAC FILTERING

The MAC (Media Access Controller) Address filter option is used to control network access based on the MAC Address of the network adapter. A MAC address is a unique ID assigned by the manufacturer of the network adapter. This feature can be configured to ALLOW or DENY network/Internet access.

## 25 - MAC FILTERING RULES

Configure MAC Filtering below:

Remaining number of rules that can be created: 25

| MAC Address |  | DHCP Client List | Schedule

Helpful Hints..
• Create a list of MAC addresses and choose whether to allow or deny them access to your network.
• Computers that have obtained an IP address from the router's DHCP server will be in the DHCP Client List. Select a device from the drop down menu and click the arrow to add that device's MAC to the list.
• Use the check box on the left to either enable or disable a particular entry.
• Use the Always drop down menu if you have previously defined a schedule in the router. If not, click on the Add New button to add one.

More...

Copyright © 2004-2007 D-Link Systems, Inc.