dlink-B4938F

Product Page: DNS-343 |  | Firmware Version: 1.03

| Setup | Advanced | Maintenance | Status | Support

- RAID
- Users / Groups
- Quotas
- Network Access
- FTP Server
- UPnP AV Server
- iTunes Server
- DHCP Server
- LLTD
- Remote Backup
- Add-ons
- Logout

# HARD DRIVE CONFIGURATION :

RAID CONFIGURATION allows you to change your hard drive configuration, or format a newly inserted hard drive. Please note that formatting a hard drive will erase any data that was stored on the hard drive.

AUTO-REBUILD CONFIGURATION allows you to enable or disable the Auto-Rebuild feature. You can also manually rebuild by clicking the Manually Rebuild Now button. Please note that rebuilding will erase all data on the newly inserted drive.

## RAID CONFIGURATION :

Current RAID Type :
| Volume_1 : RAID 5

## FORMAT THE NEW 2ND DRIVE :

## RAID CONFIGURATION :

## AUTO-REBUILD CONFIGURATION :

Vendor | Model | Serial Number | Size

Enable Auto-Rebuild
Disable Auto-Rebuild

Helpful Hints..

A RAID 1 array will degrade when one of the hard drives fails. Auto-Rebuild allows a degraded RAID 1 array to be automatically rebuilt when the failed hard drive is replaced by automatically restoring data from the existing hard drive to the newly inserted hard drive.

Copyright © 2008 D-Link Corporation/D-Link Systems, Inc.