D-LINK SYSTEMS, INC. | WIRELESS ROUTER : Advanced / Inbound Filter

Firmware Version: 1.12
Hardware Version: A2
Product Page: DIR-855

| Setup | Advanced | Tools | Status | Support

## Reboot needed

Your changes have been saved. The router must be rebooted for the changes to take effect. You can reboot now, or you can continue to make other changes and reboot later.

## Configuration Warnings

## Inbound Filter

The Inbound Filter option is an advanced method of controlling data received from the Internet. With this feature you can configure inbound data filtering rules that control data based on an IP address range.

Inbound Filters can be used for limiting access to a server on your network to a system or group of systems. Filter rules can be used with Virtual Server, Port Forwarding, or Remote Administration features.

Note: Only Administrator has access to these functionalities.

### Add Inbound Filter Rule

You cannot add more rules because the table is full.

### Add Inbound Filter Rule

Name :

Action :

Remote IP Range :

Enable | Remote IP Start | Remote IP End
--- | --- | ---

### Inbound Filter Rules List

Name | Action | Remote IP Range |  |
--- | --- | --- | --- | ---

Helpful Hints...

Give each rule a Name that is meaningful to you.

Each rule can either Allow or Deny access from the WAN.

Up to eight ranges of WAN IP addresses can be controlled by each rule. The checkbox by each IP range can be used to disable ranges already defined.

The starting and ending IP addresses are WAN-side address.

Click the Add or Update button to store a finished rule in the Rules List below.

Click the Edit icon in the Rules List to change a rule.

Click the Delete icon in the Rules List to permanently remove a rule.

More...

Copyright © 2004-2008 D-Link Systems, Inc.