D-LINK SYSTEMS, INC | WIRELESS ROUTER | ADVANCED

Product Page: DIR-451 | Hardware Version: A1 | Firmware Version: v1.03_NA

| Setup | Advanced | Tools | Status | Support

- Virtual Server
- Port Forwarding
- Application Rules
- Network Filter
- Website Filter
- Firewall Settings
- advanced Wireless
- advanced Network

# MAC Filtering :

The MAC (Media Access Controller) Address filter option is used to control network access based on the MAC Address of the network adapter. A MAC address is a unique ID assigned by the manufacturer of the network adapter. This feature can be configured to ALLOW or DENY network/Internet access.

## 20 - MAC Filtering Rules

Configure MAC Filtering below:

MAC Address |  | DHCP Client List |

Helpful Hints..
Mac Filtering:
Create a list of MAC addresses that you would either like to allow or deny access to your network.

Computer Names:
Computers that have obtained an IP address from the router's DHCP server will be in the DHCP Client List. Select a device from the drop down menu and click the arrow to add that device's MAC to the list.

Clearing an Entry:
Click the CLEAR button to remove the MAC address from the MAC Filtering list.

Copyright © 2004-2008 D-Link Systems, Inc.