D-LINK SYSTEMS, INC | WIRELESS ROUTER | HOME

Product Page: DIR-615 | Hardware Version: A1 | Firmware Version: 1.10

| Setup | Advanced | Tools | Status | Support

- Internet
- Wireless settings
- Network settings

# Network Settings :

Use this section to configure the internal network settings of your router and also to configure the built-in DHCP Server to assign IP addresses to the computers on your network. The IP Address that is configured here is the IP Address that you use to access the Web-based management interface. If you change the IP Address here, you may need to adjust your PC's network settings to access the network again.

## Router Settings :

Use this section to configure the internal network settings of your router. The IP Address that is configured here is the IP Address that you use to access the Web-based management interface. If you change the IP Address here, you may need to adjust your PC's network settings to access the network again.

Router IP Address : |
Default Subnet Mask : |
Local Domain Name : |
Enable DNS Relay : |

## DHCP Server Settings :

Use this section to configure the built-in DHCP Server to assign IP addresses to the computers on your network.

Enable DHCP Server : |
DHCP IP Address Range : | to (addresses within the LAN subnet)
DHCP Lease Time : | (minutes)

## Add DHCP Reservation :

Enable : |
Computer Name : |
IP Address : | 192 . 168 . 0 .
MAC Address : |

## DHCP Reservations List:

Enable | Computer Name | MAC Address | IP Address

## Dynamic DHCP Client List :

Computer Name | IP Address | MAC Address | Expired Time
end_user | 192.168.0.100 | 00:05:5d:ce:b3:8d | Tue Jul 31 05:45:16 2007

Helpful Hints.. If you already have a DHCP server on your network or are using static IP addresses on all the devices on your network, uncheck Enable DHCP Server to disable this feature. In order to ensure that devices on your network are always assigned the same IP address, add a DHCP Reservation for each device.

Copyright © 2004-2005 D-Link Systems, Inc.