dlink-ECEA07

Product Page: DNS-323 |  | Firmware Version: 1.09

| SETUP | ADVANCED | TOOLS | STATUS | SUPPORT

- ADMIN PASSWORD
- TIME
- SYSTEM
- FIRMWARE
- E-MAIL ALERTS
- POWER MANAGEMENT
- RAID
- DDNS
- DISK TOOLS
- LOGOUT

# HARD DRIVE CONFIGURATION :

This section allows you to setup a RAID configuration on the selected hard drives. Please note that the data stored on the drives will be erased during the formatting process.

AUTO-REBUILD CONFIGURATION allows you to enable or disable the Auto-Rebuild feature. You can also manually rebuild by clicking the Rebuild button in the RAID CONFIGURATION section. Please note that rebuilding your volume will erase all data on the newly inserted drive.

## RAID CONFIGURATION :

Current RAID Type :
| Volume_1 : Standard

## CONFIGURE THE NEW 2ND DRIVE :

## Remaining Size :

## AUTO-REBUILD CONFIGURATION :

Vendor | Model | Serial Number | Size
Seagate | ST3250310AS | 6RY3L68X | 250 GB

Enable Auto-Rebuild
Disable Auto-Rebuild

Helpful Hints..

A RAID 1 array will degrade when one of the hard drives fails. Auto-Rebuild allows a degraded RAID 1 array to be automatically rebuilt when the failed hard drive is replaced by automatically restoring data from the existing hard drive to the newly inserted hard drive.

Copyright © 2006-2009 D-Link Corporation/D-Link Systems, Inc.