DWL-3200AP

Tools

Administrator Settings
Administrator settings allow you to customize User Name and Passwords as an Administrator of . The default value of the Username is "admin" with no password entered.
User Name
Enter a password in the Access Point Password field. Type the password again in the next field to confirm it. The Password is case-sensitive ("A" is a different character than "a",) and must be between 0 and 12 characters in length.
Old Password
Enter the Old Password of the Administrator .
New Password
Enter the new password for the Administrator. The maximum number of characters to be used for passwords is 12 characters and the password is case-sensitive.
Confirm New Password
Please confirm your new password by re-enter the new password.

System Settings
User can restart to apply new settings or reset to factory default.
Apply Settings and Restart
By clicking "Restart" button, will restart and applied settings modified.
Restore Default Settings
By clicking "Restore" button, will be reset to factory default.

Firmware upgrade
User can download the latest firmware from D-Link website. Please visit http://support.dlink.com for more information.
Update firmware From Local Hard Drive
User can change firmware by browsing to the directory where the firmware is located and update it by clicking "OK".

Configuration File
Update Configuration File
User can apply specific configurations by browsing to the directory where the configuration file is located and update it by clicking "OK".
Download Configuration File
User can save configuration to local hard drive by clicking "OK".

Miscellaneous User can disable or enable Telnet function for and specify telnet duration allowed. The default value of Telnet function is "enable" with timeout default "3 Minutes".