dlink-6CE05B

Product Page: DNS-726-4 |  | Firmware Version: 1.00

| Live Video | Playback | Setup | Maintenance | Status | Help

- Menu
- Live Video
- Playback
- Setup
- Maintenance
- Status
- Logout

#
HELP MENU

- Playback

##
PLAYBACK

Play the Recorded Video
1. Be sure that you have set the schedule/ recording event first.
2. Open Internet Explorer and login the unit.
3. Click the Playback button on the top of the page.
4. Click the Open Record button.
5. The Record Display Window will show the information of the available video clips. Select the date you want to search the record from. See the manual for more details about the Record Display Window.
6. Highlight the video records that you want to review. See the Manual for more details.
7. Click the OK button.
Open Record
Click the Open Record button to access the Date-Time Panel and select the video records which you want to playback.

Settings

- Record Display
  - Calendar View: make the Record Display Window as calendar view.
  - List Control: make the Record Display Window as list control.
- Play
  - Play when open: check the option and set the system to start playing the video clip every time when a record is withdrew.
  - Auto skip when record motion only mode: check the option to set up the system to automatically skip to the points where there were motions recorded.
  - Next interval: set the interval with which the video goes forward when you click the Forward button on the control panel.
  - Previous interval: set the interval with which the video goes backward when you click the Reverse button on the control panel.
- Capture Image
  - Save in clipboard: the image will be saved in the clipboard and can be pasted on other application software.
  - Manually save the image file: you can manually select where you want to save the image, name the saved file, and choose the format you want to save the image.
  - Automatically save the image file: by pre-setting a path/URL and the image format, the system will automatically save the image accordingly when you click the Save Image button on the control panel.

Single / Quad split Screen
User can select to view single camera or 4 cameras at a time. Basic version only Supports 1 camera playback.
Full Screen
Select to display the video with full screen. Press ESC button on the keyboard can return to normal display.
Information Window
Display video date and time, cue in/ out points, time and speed.
Audio Volume Control
Adjust the sound level.
Digital Zoom
Click the icon to digital zoom in or digital zoom out the view. Every camera can use this function.
Play / Stop / Pause
Select a camera/ video and click this button to play/stop/pause a particular channel.
Speed
Click the + or - button to increase or decrease the playback speed.
Cue in / Cue out
Click the Cue In or Cue Out button to set the period for Save Video.
Step forward / Reverse
Click to pause the playback and move to next frame or last frame.
Fast forward / Reverse
Click to pause the playback and move to next minute or last minute.
Search the Recorded Video to Playback
User can refresh the Date Time Search Dialog Window or go to previous or next recording date by press the upper left corner buttons.
Record Display Window
Display the available recorded video records.
Date Time Period
Select the start and end time points that indicate the time period you would like to view after choosing cameras.
Video Preview
Check the Enable Preview option to view the selected video.
Time Table (pre-set recording schedule)
Click the icon "+" to select all channels; also click the icon "-" to deselect all channels. Finally, utilize the scale bar to modify the scale of the time table; there are two recording modes: Record Always and Record on Event, and Time Table will display these two modes by different colors.
Show Records
Show the period of recording data in Time Table.
Step 1: From the Record Display Window at the top left of the Date Time Panel, select the date you want to search the record from. The red lines shown on the time table indicate available recorded video records.
Step 2: Use color bars to differentiate recording types from each other. This will help you select video clips.
Step 3: Highlight the video clip you want to review by left-clicking and dragging the time period. You may also utilize the Start Time and End Time in Date Time Period Section after choosing camera. In addition, modify the scale of the time table with the icon or on the bottom left.
Step 4: Check the Enable Preview option to get the preview of the video you select.
Step 5: Click the camera name to increase or decrease cameras you want to playback.
Step 6: Click the OK button will begin to playback.
Note The Record Display Window can be shown in (a) calendar view or (b) list control view. To modify the setting of the record display window, click the Setting button at the right of the page. See manual for more details.
Smart Search from the Recorded Video (Pro version only)
After opening the recorded video, click the Search Mode button to obtain the Intelligent Search Tool panel. You can search unusual events during the recoding period.
There are 5 types of unusual events: General Motion, Foreign Object, Missing Object, Lose Focus, and Camera Occlusion.
General Motion
Detect all movements in the defined area.
1. Define detection zone by dragging to draw a detection zone. You may define more than one zone by repeating this step.
2. Modify the sensitivity setting by changing the slider control. Moving toward right will increase the sensitivity level, which means a relatively small movement will trigger the alarm.
3. Set the interval. Moving toward right will increase time interval so that the alarm will only be triggered when the movement lasts longer.
4. Check the Stop when found option. If uncheck, the search tool will list all the events it found, instead of stopping at the moment the event found.
5. Click the Search button.
Foreign Object
Alarm is set on when any additional object appears in the defined area on the screen.
1. Define detection zone by dragging to draw a detection zone.
2. Modify the sensitivity setting.
3. Set the Interval.
4. Check the Stop when found option. If uncheck, the search tool will list all the events it found, instead of stopping at the moment the event found.
5. Click the Search button.
Missing Object
Alarm is set on when the selected object is removed from the defined area on the screen.
1. Define detection object by dragging to draw a detection zone.
2. Modify the sensitivity setting.
3. Set the Interval.
4. Check the Stop when found option. If uncheck, the search tool will list all the events it found, instead of stopping at the moment the event found.
5. Click the Search button.
Lose Focus
System will inform you when the camera(s) lose its focus.
Camera Occlusion
Alarms when the camera is blocked.
Recorded Video Enhancement
During playback, user can click the Enhancement button to make some post processing of the video display quality.
Check the General Setting.
Apply active channel
The settings will be only applied to the selected channel.
Apply all channels The settings will be only applied to those currently shown on the screen.
Set the Filter Setting.
Visibility
Check the option and adjust the gamma value of the image to enhance the image and make it cleaner.
Sharpen Check the option to activate the function. Move the slider control to the right to sharpen the image, to the left to soften it.
Brightness Check the option to activate the function. Move the slider control to the right to make the image brighter.
Contrast Check the option to activate the function. Move the slider control to the right to increase contrast.
Grey Scale Check the option to show the record in grey scale mode so the image displays in black and white.
Stop Stop the enhancement function and close the enhancement tool. (The system will automatically back to the default settings.)
Default Back to the default settings, however, the enhancement tool still works.
OK Apply the modifications of the settings.
Save Video
Step 1: During playback, user can choose the camera that you want to save as a video clip.
Step 2: Set up the cue in and cue out points; the cue in and cue out time will be shown on the information window. Then click the Save Video button.
Step 3: Choose the folder where you want to save the file.
Step 4: Input the file name and click the Save button.
Step 5: Choose the export format.
Step 6: Choose the use profile.
Step 7: Check the Export Audio option if the video has audio and you would like to export with the video.
Step 8: Click the OK button.
Note We recommend you to export to the .asf format when saving video. In exporting to the .avi format, the frame rate will be increased when playing in the video player and there is no time stamp on the video.
Save Image
Step 1: During playback, user can choose the camera that you want to save as a picture.
Step 2: Click the Save Image button when the image you want is shown on the screen.
Step 3: Choose the folder where you want to save the file.
Step 4: Choose the folder and the format of image (BMP or JPEG) you prefer.
Step 5: Input the file name.
Step 6: Click the Save button.
Note You may skip step 3 by pre-setting a folder and format what you want to save the images. See the "Setting" option for more details.
Print Image
Step 1: During playback, user can choose the camera that you want to print a picture.
Step 2: Click the Print button when the image you want is shown on the screen.
Step 3: Set print settings.
Page Setting
Print in original size Check to have the image print in original size.
Fit the page Check to have the image fit the page.
Align Image Align the top, center or bottom.
Print Content Print the image from currently selected channel or all the channels shown on the screen.
Step 4: Click the Print button.
Backup the Recorded Video
Different from Save Video, the Backup function will save all the recorded videos during the time period you select, instead of a single video clip.
Step 1: After user use Open Record to select desired data.
Step 2: Click the Backup button.
Step 3: Set the Start Time and End Time you want to backup.
Step 4: Select the cameras you want to backup.
Step 5: Select the directory you want to save the backup data.
Step 6: Click the Backup button. The system will then begin backup process automatically.

Copyright © 2008 D-Link Corporation/D-Link Systems, Inc.