DSA-3100B Release 3.10
Release Date:  12-12-2005

Importance Notices:
 - The saved setting file, the database image file, must be applied on the same version firmware system only, due to the database compatibility issue.
 - The step of “reset to factory default” at the end of the firmware upgrade procedures is very important to ensure the new system with the proper database.

Resolved Issues:
 - To improve the firmware upgrade compatibility, the version of 3.10 is capable to be upgrade from versions of 3.01, 3.02, 3.03 B1 and 3.04 
 - To prevent the firmware upgrade operation failure from the double clicks on the Apply button, the effective click is limited on the first one only.
 - To protect the system resource, only 50 concurrent users are limited.
 - User name too long, the UI will NOT be broken any more.
 - Status/Current Users won’t be shown the same user name when quick login after logout with different users from the same PC 
 - kick out record will be shown for RADIUS user
 - the time in the history record will reflect the time zone setting 
 - Virtual server is working after expansion to 30 sets of configuration 
 - Virtual Server port setting will not be lost 
 - login for two hours the ping function is function well now. 
 - Session-timeout of the RADIUS user will not be replaced by the last RADIUS login user, reported from D-Link HQ20050601000001 
 - WAN setting now will NOT take effect immediately without restart 
 - IP-PNP for Public LAN under NAT is working now
 - PRONTO mode now will not force the Public IP to change to 192.168.4.x 
 - Bandwidth control now match the actual data-rate 
 - Now, there is no duplicate kick out record in Traffic History
 - WAN port DNS server IP setting now will display the correct IP 
 - RADIUS now will send 'Acct-Terminate-Cause' 
 - The Change password function from SSH menu now is also changing the password for admin login from WEB UI, even after done with the restore db.
 - PPPoE now is working well when WAN fail function enabled 
 - DHCP relay now is working well on LAN if relaying a server from WAN port
 - Airpath now is working well with login schedule enabled.
 - Restore db with a different admin password, now, will NOT redirect the page to the admin login.