   LAN Server 4.0

   [1].Introduction:
   ----------------
      This document describes the procedure to install NDIS driver on DOS
      LAN Requester for D-Link DFE-538TX 10/100 Adapter.

   Location of Driver:  \NDIS2\DOS\DLKRTS.DOS  (for DOS LAN Services)
                        
   [2].Installing driver procedure on DOS LAN Requester :
   -----------------------------------------------------
      Before you start with the installation process, make sure that
      DOS LAN Services is properly installed. Similarly, your adapter
      should also be properly installed in your client PC.

      1. Copy DLKRTS.DOS from your Driver disk (EX: E:\NDIS2\DOS)
         to DOS LAN Services subdirectory C:\DLS .

      2. Under DOS LAN Requester subdirectory C:\DLS, run INSTALL

      3. The screen display some description. If it's correct, move
         highlight to "The listed options are correct" item ,then press
         ENTER.

      4. Move highlight to "Network Card", then press ENTER.

      5. Select "Change driver for network card." item, then press ENTER.

      6. Select "Network card not shown in list below..", then press ENTER.

      7. Insert the DFE-538TX driver disk into CD-ROM drive,and 
         specify your pathname, EX: E:\NDIS2\DOS, then press ENTER.

      8. D-Link DFE-538TX driver is now installed on your computer, reboot
         your computer.

    [3].A sample PROTOCOL.INI file:
    -------------------------------

         [DLKRTL]
         DriverName=DLKRTS$
         EtherID=@52544C111111  ;This keyword is used to desinate a DFE-538TX
                                ;adapter by assigning it's ethernet ID
                                ;when more than one adapters exist on one
                                ; system.

         Medium= _Auto, _10Half, _10Full, _100half, _100Full      
                            ;This keyword is used to force DFE-538TX adapter
                            ;to speed 10M or 100M mode. If not present,
                            ;the driver will auto-detect the speed.
                            