   LAN Manager Workstation/Server

   Introduction:
   -------------
   This document describes the procedure to setup LAN  Manager 2.1
   Workstation/Server driver for D-Link DFE-538TX 10/100 Adapter.

   Location of Driver: \MSLANMAN.DOS\DRIVERS\ETHERNET\DLKRTS\DLKRTS.DOS
                      

   Sample Configuration Files:
   ---------------------------
   CONFIG.SYS :

      DEVICE=C:\LANMAN.DOS\DRIVERS\PROTMAN\PROTMAN.DOS /I:C:\LANMAN.DOS
      DEVICE=C:\LANMAN.DOS\DRIVERS\ETHERNET\DLKRTS\DLKRTS.DOS

   PROTOCOL.INI (will contain):

      [DLKRTL]
      ; DFE-538TX RPOTOCOL.INI SAMPLE
      DriverName=DLKRTS$
      EtherID=@52544C111111  ;This keyword is used to desinate a DFE-538TX
                             ;adapter by assigning its ethernet ID
                             ;when more than one adapters exist on one
                             ; system.

      Medium= _Auto, _10Half, _10Full, _100half, _100Full      
                         ;This keyword is used to force DFE-538TX adapter
                         ;to speed 10M or 100M mode. If not present,
                         ;the driver will auto-detect the speed.


   Setup driver procedures on LAN Manager workstation/server :
   -----------------------------------------------------------
   Before you start with the installation process, make sure that the
   adapter is properly installed and configured. Make sure your
   Microsoft LAN Manager is properly installed.

   1. Run the appropriate Microsoft Lan Manager SETUP for computer you
      are setting up.(DOS, OS/2 or OS/2 Server). Select "Configuration"
      item ,(the driver isn't included on the Lan Manager disk)
      and insert the DFE-538TX driver disk, select the DFE-538TX
      driver and follow the directions.

   2. When completed, reboot your computer.

   Installing Multiple LAN Adapters:
   ---------------------------------

   To Follow Setup driver Procedure and add two adapter,

   Under  DOS  mode, you can modify the EtherID or BusNo+DeviceNo
   Keyword field in file C:\LANMAN\PROTOCOL.INI.
