
            D-Link DFE-570TX FAST Ethernet Server Adapter Installation
                            for Windows 2000

 Getting Started
 ---------------

    The Windows 2000 installation CD is needed to complete this
    installation.

    Windows 2000 Installation Procedure
    -----------------------------------

    Update driver from diskette/CD-ROM
    ----------------------------------
    The following steps can help you update the bundled driver to
    the one in the Adapter Drivers Diskette/CD-ROM.

     1. Open Control Panel, double click "System" icon to open System
        Properties.

     2. In the "Hardware" sheet, you can see the "Device Manager" bottum.
        Click to open Device Manager.

     3. Use the tool bar to make sure you "View" "Devices by type".
        Than you will able to find

        Intel 21143 Based PCI Fast Ethernet Adapter

        in "Network Adapters" group. Double click it to open its property.

     4. In the "Driver" sheet of the adapter's properties, there is a button
        named "Update Driver". Click it, the Upgrade Device Driver Wizard
        will show up to help updating the driver.

     The following steps will lead you through the wizard ...

     1. The first page is the welcome messages, click "Next" to continue.

     2. Select "Search for a suitable driver for my device (recommanded)",
        and click "Next".

     3. Check "Specify a location" only. Click "Next" to continue.

     4. Specify the path.
        (A:\ , assume A: is floppy drive)
        (D:\ , assume D: is CD drive) 
        
     5. The wizard will find the specified driver.

        D-Link DFE-570TX PCI Fast Ethernet Server Adapter

        Click "Next" to continue.

     6. The wizard will copy and load the driver, than you will see "Finish"
        bottum. Click it and it's done.
