    ‪©Copyright 2008-2010 Marvell®.‬
    All rights reserved.

    setup.htm created 2010-01-14

    Readme File for D-Link Corporation Control Program v11.11.17.3

    Supporting: D-Link DGE-5xx Gigabit Ethernet Adapters

    This package contains the following software components:

    - Network Configuration Utility v11.11.4.3 (32 bit)
    - Network Configuration Utility v11.11.4.3 (64 bit)

    - NDIS5.1 Miniport Driver v11.22.3.3 for Windows XP/Server 2003 (32 bit)
    - NDIS5.1 Miniport Driver v11.22.3.3 for Windows XP/Server 2003 (64 bit)
    - NDIS6 Miniport Driver v11.22.3.3 for Windows Vista/Server 2008 (32 bit)
    - NDIS6 Miniport Driver v11.22.3.3 for Windows Vista/Server 2008 (64 bit)
    - NDIS6.2 Miniport Driver v11.22.3.3 for Windows 7 (32 bit)
    - NDIS6.2 Miniport Driver v11.22.3.3 for Windows 7/Server 2008 R2 (64 bit)

    - Link Aggregation Protocol Driver v11.10.3.3 for Windows XP/Server 2003 (32 bit)
    - Link Aggregation Protocol Driver v11.10.3.3 for Windows Vista/Server 2008 (32 bit)
    - Link Aggregation Protocol Driver v11.10.3.3 for Windows 7 (32 bit)
    - Link Aggregation Protocol Driver v11.10.3.3 for Windows XP/Server 2003 (64 bit)
    - Link Aggregation Protocol Driver v11.10.3.3 for Windows Vista/Server 2008 (64 bit)
    - Link Aggregation Protocol Driver v11.10.3.3 for Windows 7/Server 2008 R2 (64 bit)

    - VLAN Protocol Driver v11.10.1.3 for Windows XP/Server 2003 (32 bit)
    - VLAN Protocol Driver v11.10.1.3 for Windows Vista/Server 2008 (32 bit)
    - VLAN Protocol Driver v11.10.1.3 for Windows 7 (32 bit)
    - VLAN Protocol Driver v11.10.1.3 for Windows XP/Server 2003 (64 bit)
    - VLAN Protocol Driver v11.10.1.3 for Windows Vista/Server 2008 (64 bit)
    - VLAN Protocol Driver v11.10.1.3 for Windows 7/Server 2008 R2 (64 bit)

# This file contains

1 Overview
2 Required Files
3 Installer options
4 Installation
5 Uninstallation
6 Team/VLAN Limitations
7 Troubleshooting

## 1 Overview

    The D-Link Corporation Control Program contains the Yukon® network driver and
    the D-Link CCP, that allows you to configure teams and VLANs, as well as to set
    driver parameters for the Yukon network adapters.

    The software package can be installed on a system with one of the following
    operating systems:

    Windows XP/Server 2003 (32 bit), Windows XP/Server 2003 (64 bit), Windows
    Vista/Server 2008 (32 bit), Windows Vista/Server 2008 (64 bit), Windows 7 (32
    bit), Windows 7/Server 2008 R2 (64 bit)

## 2 Required Files

    To install the software package, the following file is required:

        setup.exe

## 3 Installer options

    Valid command line parameters for the installer are:

    /? to show help
    /S for silent installation
    /U for uninstallation if the package is installed
       (cannot be combined with /S)

    Examples:
    Silent Installation
      setup.exe  /S
      will silently install the package, any confirmation requested will
      automatically be given.

## 4 Installation

    NOTE: To install the software package, you must be logged in
          as a user with administrative rights.

    To install D-Link Corporation Control Program, proceed as follows:

    1. Execute the file setup.exe.

    2. Follow the instructions displayed during the installation procedure.

    OR

    1. Open a command shell (CMD.EXE).

    2. Enter
    	setup.exe /S  for silent installation

## 5 Uninstallation

    NOTE: To uninstall the software package, you must be logged in
          as a user with administrative rights.

    To uninstall D-Link Corporation Control Program, proceed as follows:

    1. Open "Control Panel".

    2.  Before Windows Vista (XP/Server 2003):
    	Choose 	"Add or Remove Programs"
    	Select 	"D-Link Corporation Control Program" and click the "Change/Remove" button.

        Starting with Windows Vista (Vista/Win7):
    	Choose "Programs | Programs and Features | Uninstall a program"
    	Double-click "D-Link Corporation Control Program"

    OR

    1. Open a command shell (CMD.EXE).

    2. Enter
    	setup.exe /U to invoke uninstallation

## 6 Team/VLAN Limitations

    - It is not possible to add an adapter port that is already part of a VLAN
      to a team. You must remove the VLAN from this adapter port first. It is not
      possible to configure the same port to a VLAN and to a team.

    - Fast Ethernet adapters cannot be grouped into a team together with Gigabit
      Ethernet adapters.

    - For basic teaming, IPv6 is not supported.

    - Starting with Windows Vista, always both ports of a dual port adapter are added
      to the team.

## 7 Troubleshooting

    If you should encounter any problems with the installation or uninstallation of
    D-Link Corporation Control Program, send the log file "ykinstutil.log" (can be
    found in the Windows directory) to our technical support.

    If you should encounter any problems with the Corporation Control Program, please
    re-read the instructions above and the documentation supplied with the operating
    system carefully.

    If your particular problem is not listed or the error persists, please send your
    system event log file (can be found in Windows Event Viewer) or at least the
    event ID number and the logging data of the event generated by the D-Link CCP to
    our technical support.

    *** End of Readme File ***