DHN-910 Introduction
Kit Contents
Step 1: Network Planning
Step 2: Installing Adapters
Step 3: Installing Cables
Step 4: Installing Software
Networking Basics
Troubleshooting
Step 4: Installing Software Windows 98 and Windows 95 (OSR2.x) Drivers Since the DHN-520 is Plug-and-Play, Windows 98 and Windows 95 (OSR2.x) will recognize that you have added a Network Adapter and request that you provide the necessary device driver. The Windows 98 or Windows 95 (OSR2.x) installation disks or CD will be needed to complete this installation. Windows 98 and Windows 95 (OSR2.x) are referenced as Windows 95/98 below. A. Plug in and power ON your computer. B. Windows 95/98 will detect the new hardware, and will launch the Add New Hardware Wizard. The wizard will find your new "PCI Network Controller" or Network Adapter.
© 1999 D-Link Systems, Inc. All rights reserved.